|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Sr. No** | **Frequency range GHz** | **polarization** | **Gain** | **Beam width (3dB) deg.** | **VSWR** | **Isolation (dB)** | **Probable OEMs** | **Qty** |
| **1** | 0.5-2 encapsulated in radomes | Dual Circular | -6 to 6 dBiC | 62 to 102 | <1.5:1 | TBD | 1. STEATITE Q- par, UK  2.COBHAM, UK | 06 |