|  |  |  |
| --- | --- | --- |
| **Sr#** | **Description** | **Qty** |
| 1 | **Liquid Ring Compressor**-           Gas Handled: varying composition of Hydrocarbons and Nitrogen, Ethylene Dichloride (EDC), Benzene, Chloroform, Carbon Tetrachloride-           Molecular Weight: 99 (for design basis)-           Suction Pressure: 1.5 kPa (g)-           Discharge Pressure: 70 kPa (g)-           Suction Temperature: 70 deg C-           Discharge Temperature: vendor to specify-           Capacity/Flow: 560 m3/hr (Max)(the unit should be able to operate on total recycle also)-           Sealing Fluid: Water-           Preferred Material of Construction: Vendor to specify (should be compatible with the gases handled and traces of HCl) | One |