**BOILER FEED WATER PUMPS**

|  |  |
| --- | --- |
| **Pump Normal Capacity** | **96 T/H** |
| **Head** | **80 Bar g** |
| **Temperature** | **105 ºC** |
| **Pump type** | **Multistage-Radial split casing** |
| **Bearings** | **Roller** |
| **Lubrication** | **Grease** |
| **Motor Power** | **…..KW (Vendor To Advise)** |
| **Power source** | **400 V; 50 Hz** |
| **Motor protection class** | **IP 55,, nonhazardous** |
| **Quantity** | **03 Nos.** |