:

|  |  |  |
| --- | --- | --- |
| **Sr#** | **Description** | **Qty** |
| 1 | **Cylindrical Parallel Shaft Gear Reducer**           ZSY 160 – III (Right) with back stopper           Without motor           Input Power: 5.5 kW           Ratio: 31.5           Output Speed: 75 rpm           Input Speed: 1420 rpm | 2 |
| 2 | **Cylindrical Parallel Shaft Gear Reducer**           ZSY 160 – IV (Left) with back stopper           Without motor           Input Power: 5.5 kW           Ratio: 31.5           Output Speed: 75 rpm           Input Speed: 1440 rpm | 1 |
| 3 | **Cylindrical Parallel Shaft Gear Reducer**           ZSY 180 – III (Right) with back stopper           Without Motor           Input Power: 7.5 kW           Ratio: 31.5           Output Speed: 75 rpm           Input Speed: 1440 rpm | 1 |
| 4 | **Cyclo Drive Speed Reducer**           XWD 3-6-59 Reducer with Motor           IP55, 50Hz, 400V           Rotate Speed: 18 | 2 |