:

|  |  |  |
| --- | --- | --- |
| **Sr#** | **Description** | **Qty** |
| 1 | **Cylindrical Parallel Shaft Gear Reducer**         ZSY 160 – III (Right) with back stopper         Without motor         Input Power: 5.5 kW         Ratio: 31.5         Output Speed: 75 rpm         Input Speed: 1420 rpm | 2 |
| 2 | **Cylindrical Parallel Shaft Gear Reducer**         ZSY 160 – IV (Left) with back stopper         Without motor         Input Power: 5.5 kW         Ratio: 31.5         Output Speed: 75 rpm         Input Speed: 1440 rpm | 1 |
| 3 | **Cylindrical Parallel Shaft Gear Reducer**         ZSY 180 – III (Right) with back stopper         Without Motor         Input Power: 7.5 kW         Ratio: 31.5         Output Speed: 75 rpm         Input Speed: 1440 rpm | 1 |
| 4 | **Cyclo Drive Speed Reducer**         XWD 3-6-59 Reducer with Motor         IP55, 50Hz, 400V         Rotate Speed: 18 | 2 |