|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Sr. No** | **Description** | **Model** | **Make** | **Qty** |
| **1** | **Differential Pressure Switches**  LDD: Differential pressure control, two independently adjustable set points, fixed dead band  N4: NEMA 4, 4 X L-Series: Epoxy coated, Dei Cast Aluminum, IP66  KK: Dual Switch Narrow Dead band  Actuator Seal: Buna-N (-18….65oC) (B)  1/4 NPT Female and ½ NPT Male Combination pressure only  XFS: Factory adjusted set point  TM: 2" pipe mounting bracket  Range: 0–4 Bar  Set Point: 380 mbar decreasing, 2 bar increasing | **LDD-N4-KK-B-06-XFS-TM-0/4Bar or Equivalent** | **Ashcroft, USA**  **Or Equivalent** | **140** |