|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Sr. No** | **Description** | **Model** | **Make** | **Qty** |
| **1** | **Differential Pressure Switches**LDD: Differential pressure control, two independently adjustable set points, fixed dead bandN4: NEMA 4, 4 X L-Series: Epoxy coated, Dei Cast Aluminum, IP66KK: Dual Switch Narrow Dead bandActuator Seal: Buna-N (-18….65oC) (B)1/4 NPT Female and ½ NPT Male Combination pressure only XFS: Factory adjusted set point TM: 2" pipe mounting bracketRange: 0–4 BarSet Point: 380 mbar decreasing, 2 bar increasing |       **LDD-N4-KK-B-06-XFS-TM-0/4Bar or Equivalent** |        **Ashcroft, USA****Or Equivalent** | **140** |