|  |  |  |  |
| --- | --- | --- | --- |
| **Item#** | **Item description** | **UOM** | **QTY** |
| 1. | BACK SHELL, STRAIN RELIEF SIZE 14 ALUMINUM P/N M85049/47W14 Manufacturer: GLENAIR OEM PART NO.:M85049/47W14 | No. | 20 |
| 2. | CONNECTOR; 37PIN BACK SHELL SIZE 14 Manufacturer: SUNBANK OEM PART NO.:M85049/47SW14 | No. | 20 |
| 3. | CONNECTOR; SOCKET 37 PIN SHELL SIZE-14 CABLE MOUNT Manufacturer: CONESYS AERO ELECTRIC OEM PART NO.:MS27484T14B35S | No. | 20 |
| 4. | CONNECTOR; PLUG 37 PIN SHELL SIZE-14 BOX MOUNT Manufacturer: CONESYS AERO ELECTRIC OEM PART NO.:MS27508E14B35P | No. | 20 |
| 5. | PIN CONTACT; STANDARD PCB PIN SIZE 22D Manufacturer: AMPHENOL OEM PART NO.: 900245-91 | No. | 1000 |
| 6. | SOCKET; STR PCB 24WAY (2ROW 12+12) 2MM PITCH DIL Manufacturer: HARWIN OEM PART NO.:M22-7141242 | No. | 65 |
| 7. | CONNECTOR; COAXIAL PLUG 50 OHM R/A P/N 1-1634002-0 Manufacturer: TE CONNECTIVITY OEM PART NO.:1-1634002-0 | No. | 20 |
| 8. | CONNECTOR; PLUG TNC COAXIAL STRAIGHT 50R RG558 P/N 1-1478415-0 Manufacturer: TE CONNECTIVITY OEM PART NO.:1-1478415-0 | No. | 20 |
| 9. | TMMB MOUNTING BRACKET; ALUMINIIUM ALLOY WITH SST LOCKING NUTS SHELL SIZE14 Manufacturer: MILNEC OEM PART NO.:TMMB-14-C | No. | 20 |
| 10. | GAP PAD; STANDARD THICKNESS AVAILABLE :0.25'' Manufacturer: BERGQUIST OEM PART NO.:GPVOUS-0.250-AC-0816-NA | No. | 10 |
| 11. | WIRE; PTFE A RED 7/0.2MM 24AWG 100M Manufacturer: BRAND REX OEM PART NO.:SPC00443A001 100M | No. | 02 ROLLS |
| 12. | WIRE; PTFE A BLACK 7/0.2MM 100M P/N SPC00443A002 100M Manufacturer: BRAND REX OEM PART NO.:SPC00443A002 100M | No. | 02 ROLLS |
| 13. | WIRE; PTFE 'A' BLACK 19/0.15MM 22AWG 100M Manufacturer: BRAND REX OEM PART NO.:SPC00444A002 100M | No. | 02 ROLLS |